Net         Name        X Coord     Y Coord     Side        Hole Size   Type        
+5V_PROT    TP22-1         9.625mm       3.3mm  Top                0mm  Surface mount
GND_D       TP7-1          8.357mm     3.317mm  Top                0mm  Surface mount
+3.3V_REF   TP10-1         8.357mm     7.127mm  Top                0mm  Surface mount
+1.8V_MAG_CTTP9-1          8.357mm     5.857mm  Top                0mm  Surface mount
+5V_D       TP14-1         9.627mm     2.047mm  Top                0mm  Surface mount
+3.3V_D     TP6-1          9.627mm     7.127mm  Top                0mm  Surface mount
+5V_FBK     TP17-1         9.627mm     5.857mm  Top                0mm  Surface mount
\ETH1_LED_LINKSTATUS_ANODETP5-1            2.5mm      2.54mm  Top                0mm  Surface mount
\ETH0_LED_LINKSTATUS_ANODETP1-1            2.5mm     -2.54mm  Top                0mm  Surface mount
FAULT_SIGNAL_ANODETP3-1            2.5mm         0mm  Top                0mm  Surface mount
ECAT_CAN_RUN_ANODETP2-1            2.5mm     -1.27mm  Top                0mm  Surface mount
ECAT_CAN_ERR_ANODETP4-1            2.5mm      1.27mm  Top                0mm  Surface mount
\STO/SAFE_IN_ATP11-1         8.357mm     8.397mm  Top                0mm  Surface mount
+5V_SAFE    TP20-1         9.627mm     9.667mm  Top                0mm  Surface mount
\STO/SAFE_IN_BTP12-1         8.357mm     9.667mm  Top                0mm  Surface mount
1.65V_REF   TP8-1          8.357mm     4.587mm  Top                0mm  Surface mount
GND_D       TP13-1         8.357mm    10.937mm  Top                0mm  Surface mount
PWM_BRAKE   TP19-1         9.627mm     8.397mm  Top                0mm  Surface mount
3.3V_FBK    TP15-1         8.357mm     2.047mm  Top                0mm  Surface mount
GND_D       TP18-1         9.627mm    10.937mm  Top                0mm  Surface mount
GND_D       TP16-1         9.627mm     4.587mm  Top                0mm  Surface mount
